Author: jim wainscott

P16
3-2006

Appliance Specifications Sheet

APPLIANCE CUT-OUT FORM FOR CABINETS

PLEASE NOTE: APPLIANCE CABINETS WILL NOT BE PRODUCED WITHOUT MANUFACTURER’S SPECIFICATIONS AND COMPLETED APPLIANCE SPECIFICATIONS SHEET.

NOTE: MAXIMUM CUT OUT WIDTH IS 1¾” LESS THAN CABINET WIDTH ON FRAMED CABINETRY.
NO CUT OUT ON FRAMELESS - FILL IN ONLY.
PLEASE INCLUDE TRIM KIT OVERLAY. IF NO INFORMATION ON TRIM KITS IS PROVIDED,
YOUR CABINET WILL BE MADE WITH OUR STANDARD REVEALS.

DEALER___________________________INVOICE #_______________________JOB NAME_______________________
MANUFACTURER______________________________MODEL#_____________________

FILL IN OVER ALL HEIGHT AND WIDTH ON DRAWINGS

MWTC__________

MWOC___________

OC_____________

OCD_____________

OCWD___________

A_____________
B_____________

RC__________

A_____________
B_____________
C_____________
D_____________

A_____________
B_____________

A_____________
B_____________

A_____________
B_____________
C_____________
D_____________

ACCORDING TO THE NATIONAL KITCHEN AND BATH ASSOCIATION, THE IDEAL LOCATION FOR THE BOTTOM OF A MICROWAVE OVEN IS 3” BELOW THE PRINCIPAL USER’S SHOULDER BUT NO MORE THAN 54” ABOVE THE FINISHED FLOOR. IF THE MICROWAVE OVEN IS PLACED BELOW THE COUNTER TOP, THE MICROWAVE OVEN BOTTOM MUST BE AT LEAST 15” OFF THE FINISHED FLOOR. THE NKBA ALSO RECCOMENDS A 15” X 16” LANDING AREA ADJACENT TO AN OVEN OR MICROWAVE OVEN.

A_____________
B_____________

PennvilleCabinetry.com Office: 260.726.9357 Fax: 260.726.7044