Author: jim wainscott

P18
3-2006

Appliance Specifications Sheet

REFRIGERATOR DOOR PANELS - FRAMED

PLEASE NOTE: APPLIANCE PANELS WILL NOT BE PRODUCED WITHOUT MANUFACTURER’S SPECIFICATIONS AND COMPLETED APPLIANCE SPECIFICATIONS SHEET.

PANEL CONSTRUCTION IS ¼” PLYWOOD BACKER PANEL WITH ¾” OR 1” DOOR ATTACHED.

DEALER___________________________INVOICE #_______________________JOB NAME_______________________
MANUFACTURER______________________________MODEL#_____________________

REFRIGERATOR DOOR PANEL ORDER AS RDP.

FILL IN OVER ALL HEIGHT AND WIDTH ON DRAWINGS

A

A

B

A

C

B

B

Please specify dispenser cut out size and location.

Reveals will be 2” on handle side and ¾” balance unless otherwise specified.

PANEL “A” REVEALS:
Left:______________
Right:_____________
Top:______________
Bottom: ___________

PANEL “B” REVEALS:
Left:______________
Right:_____________
Top:______________
Bottom: ___________

PANEL “C” REVEALS:
Left:______________
Right:_____________
Top:______________
Bottom: ___________

REFRIGERATOR GRILL PANELS
ORDER AS RGP

UNDER COUNTER REFRIGERATOR PANELS
TRASH COMPACTOR DOOR PANELS
ORDER AS URDP OR TCDP

D

Reveals ¾” ON ALL SIDES unless otherwise specified.

PANEL “D” REVEALS:
Left:______________
Right:_____________
Top:______________
Bottom: ___________

Reveals ¾” ON ALL SIDES unless
otherwise
specified.

PANEL “E” REVEALS:
Left:______________
Right:_____________
Top:______________
Bottom: ___________

E

PennvilleCabinetry.com Office: 260.726.9357 Fax: 260.726.7044