Author: jim wainscott

Appliance Specifications Sheet

P19
3-2006

REFRIGERATOR DOOR PANELS -OVERLAY

PLEASE NOTE: APPLIANCE PANELS WILL NOT BE PRODUCED WITHOUT MANUFACTURER’S SPECIFICATIONS AND COMPLETED APPLIANCE SPECIFICATIONS SHEET.

PANEL CONSTRUCTION IS ¾” OR 1” DOOR WITH ⅛” GROOVE ¼” UP FROM BACK FOR TRIM KIT.

DEALER___________________________INVOICE #_______________________JOB NAME_______________________
MANUFACTURER______________________________MODEL#_____________________

Pennville will size the panels accordingly based on the dimensions you specify and compare them to the manufacturer’s specs. FILL IN OVER ALL HEIGHT AND WIDTH ON DRAWINGS.

REFRIGERATOR DOOR PANELS ORDER AS RDPOV.

INTEGRATED REFRIGERATOR DOOR PANELS
ORDER AS IRDP.

A

PANELS DO NOT NEED TO BE ORDERED
SEPERATELY FOR
SUB ZERO CABINETS
Panel “a” should be ordered as a door only.
Maximum width is 36”.
Will have center stile

Please specify dispenser cut out size and location.
Reveals will be 2” on handle side and ¾” balance unless otherwise specified.

B

C

Panels “b” and “c” should be ordered as drawer fronts only.
Maximum width is 36”.

UNDER COUNTER REFRIGERATOR PANELS
OR TRASH COMPACTOR PANELS
ORDER AS URDPOV OR TCDPOV

REFRIGERATOR GRILL PANELS

ORDER AS RGPOV

MODEL # _________________

PANEL CONSTRUCTION CONSISTS OF ¾” DOOR ONLY.

IS THIS FRAME TO BE USED ON A WINE REFRIGERATOR?
YES_____ NO______

PennvilleCabinetry.com Office: 260.726.9357 Fax: 260.726.7044