Author: jim wainscott

Appliance Specifications Sheet

P17
3-2006

APPLIANCE CUT-OUT FORM FOR CABINETS

PLEASE NOTE: APPLIANCE CABINETS WILL NOT BE PRODUCED WITHOUT MANUFACTURER’S SPECIFICATIONS AND COMPLETED APPLIANCE SPECIFICATIONS SHEET.

NOTE: MAXIMUM CUT OUT WIDTH IS 1¾” LESS THAN CABINET WIDTH ON FRAMED CABINETRY.
NO CUT OUT ON FRAMELESS - FILL IN ONLY.
PLEASE INCLUDE TRIM KIT OVERLAY. IF NO INFORMATION ON TRIM KITS IS PROVIDED,
YOUR CABINET WILL BE MADE WITH OUR STANDARD REVEALS.

DEALER___________________________INVOICE #_______________________JOB NAME_______________________
MANUFACTURER______________________________MODEL#_____________________

FILL IN OVER ALL HEIGHT AND WIDTH ON DRAWINGS

MS ______________

MWC_____________
DMWC____________

MWC1D__________
DMWC1D__________

MWCT____________

A_____________
B_____________
C_____________

OB_______________

A_____________
B_____________

DIR______________

A_____________
B_____________

DIRD_____________

A_____________
B_____________

BMWC___________
BMWCD__________
DWC_____________
__

A_____________
B_____________

A_____________
B_____________

A_____________
B_____________

A_____________
B_____________

WDB______________

ASCTB____________
RASCTB___________

A_____________
B_____________

A_____________
B_____________

PennvilleCabinetry.com Office: 260.726.9357 Fax: 260.726.7044