Author: jim wainscott

First Page Of ______________
Order Form c
Quote Form c

Order Form Revision March 1, 2006

Date - - 200____

600 East Votaw Street
P.O. Box 1266
Portland, Indiana 47371

Phone (260)726-9357
Fax (260)726-7044
www.PennvilleCabinetry.com

ORDERED BY:________________________________________________ DEALER’S P.O.#:__________________________________________________
BILL TO: ______________________________________________________ SHIP TO:________________________________________________________
_____________________________________________________________________ ______________________________________________________________________
______________________________________________________________ ________________________________________________________________
PHONE:________________________ MOBILE:_______________________ PHONE:________________________ MOBILE:________________________
FAX:___________________________ JOB NAME:______________________________________________________

COLLECTION:
c PENNVILLE-Totally custom face frame
Face frame opening height for top drawer.
c 4-1/2” standard
c 5-1/2” Pennville only
c STANFORD-Limited custom face frame
c EUROPENN-Custom plywood frameless

WOOD SPECIES:
c OAK
c KNOTTY OAK
c PECAN
c DISTRESSED PINE
c MAPLE (ADD 10%)
c CHERRY (ADD 10%)
c LYPTUS (ADD 10%)
c QUARTER SAWN OAK (ADD 10%)
c WALNUT (ADD 10%)
c CUSTOM — CALL FOR QUOTE QUOTE
____________________

SHEEN:
cLOW SHEEN c REGULAR SHEEN
20 SHEEN 60 SHEEN
2

HARDWARE:
c NONE DOORS: QTY:
c NO DRILL
c DRILL DRAWERS: QTY:

EXTERIOR FINISH OF STAIN, PAINT, OR
STANDARD SPECIALTY FINISH:
FOR CUSTOM SPECIALTY FINISHES SEE BELOW
SPECIALTY FINISHES REQUIRE A SIGNED DISCLAIMER WITH YOUR ORDER
____________________________________________________________
____________________________________________________________
____________________________________________________________

DOOR STYLE:
WALLS:________________ BASES:________________
EDGE#: ____________________
DRAWER STYLE: ___________________________
EDGE#: _______________ ____
CENTER PANEL OPTIONS (405, 415, 431 ONLY)
c COVE RAISE
c STRAIGHT
c WATERFALL
c LOUIS XIII RAISE
If center panel is not marked,
cove raise will be used
INSET OPTIONS:
c BEADED
c FLUSH
c MISSION
DOOR THICKNESS:
c 4/4 (ACTUAL DOOR IS 3/4” THICK)
c 5/4 (ACTUAL DOOR IS 1” THICK)
IF DOOR THICKNESS IS NOT MARKED
4/4 WILL BE USED

INTERIOR FINISH:
c CLEAR BIRCH (STANDARD ON STAINS, 20% UPCHARGE ON PAINT)
c PAINTED BIRCH (STANDARD ON PAINTS, 20% UPCHARGE ON STAINS)
c STAINED BIRCH (5% UP CHARGE ON STAINS, 25% UPCHARGE ON PAINTS)

HINGES:
KNIFE
c ANT. BRASS
c POLISHED BRASS
c NICKEL
DEMOUNTABLE
c ANT. BRASS
EUROPEAN
c FULL OVERLAY
c ½” OVERLAY
INSET REQUIRES A SIGNED DISCLAIMER WITH YOUR ORDER
c CONCEALED EURO INSET
c MORTISE W/ FINIAL ANTIQUE BRASS
c MORTISE W/ FINIAL RUSTIC BRONZE
c MORTISE W/ OUT FINIAL RUSTIC BRONZE
c MORTISE W/ FINIAL POLISHED CHROME
c MORTISE W/ FINIAL WROUGHT IRON
c MORTISE W/FINIAL SATIN SILVER
c MORTISE W/OUT FINIAL SATIN SILVER

ANTIQUING ORDER PROCESS: ROCK DISTRESSING ORDER PROCESS: GLAZING ORDER PROCESS: WASHING ORDER PROCESS:
35% UPCHARGE 25% UPCHARGE 15% UPCHARGE 10% UPCHARGE
BASE STAIN_________________ BASE STAIN_________________ BASE STAIN_______________ BASE STAIN______________
PAINT_______________________ PAINT______________________ GLAZE____________________ WASHING________________
LIGHT MEDIUM OR LIGHT, MEDIUM OR LIGHT OR SPECKLING 5% UPCHARGE
HEAVY ANTIQUING___________ HEAVY ROCK DIST.__________ HEAVY GLAZING____________ _________________________
GLAZE OR WASH_____________ GLAZE OR WASH____________ SPECKLING 5% UPCHARGE
FINISH OF GLAZE FINISH OF GLAZE _________________________ CRACKLE ORDER PROCESS:
OR WASH____________________ OR WASH__________________ 15% Upcharge
SPECKLING__________________ SPECKLING_________________ ____________________________
LIGHT, MEDIUM, HEAVY
OR NO ROCK DIST.____________

SPECIAL COMMENTS:
____________________________________________________________________________________________
____________________________________________________________________________________________
____________________________________________________________________________________________
____________________________________________________________________________________________
____________________________________________________________________________________________
____________________________________________________________________________________________
____________________________________________________________________________________________

Pennville warrants its cabinets against failure or defects for a full ten years after purchase. It warrants its drawer slides and hinges for life provided the cabinet is not altered or damaged from abuse. No other warranties are provided. If items are defective Pennville will replace or repair them at its option and expense (upon receipt of the defective item F.O.B. the factory). No other provision whether written or verbal shall be deemed material to this contract unless in writing and included herein. Dealers are responsible for any cost Pennville incurs due to a change order 72 hours after the dealer has received an acknowledgement. Should Pennville incur any attorney’s fees and costs in enforcing this contract, then it is agreed that dealer shall be responsible to reimburse Pennville for such expenses.

AUTHORIZED SIGNATURE:
__________________________________

PennvilleCabinetry.com Office: 260.726.9357 Fax: 260.726.7044